use ota to flash this firmware, after it finish, the ota password will change to "all-things-in-their-being-are-good-for-something", which match the yaml source.  
so you can make you own firmware base on our yaml.  

good luck with that.

we should make more doc soon. 